Title: DATA VALUE Logo__1__Graphic NOT FOUND
Author: Dirk Maximovic
Last saved by: Gregor Korb
Company: Korb Minrealölhandel

Product Name:   MOBIL VACTRA OIL NO. 1
 Revision Date:  22Oct2008 
Page  of    

______________________________________________________________________________________________________________________

SAFETY DATA SHEET

SECTION 1 | PRODUCT AND COMPANY IDENTIFICATION

As of the revision date above, this (M)SDS meets the regulations in the United Kingdom & Ireland.
PRODUCT
Product Name:     MOBIL VACTRA OIL NO. 1
Product Description:	   Base Oil and Additives
Product Code: 		   201560901010,   400231,   600486-60
Intended Use:  		 Lubricant
 
COMPANY IDENTIFICATION
Supplier:		EXXONMOBIL LUBRICANTS & SPECIALTIES EUROPE, A DIVISION OF EXXONMOBIL PETROLEUM & CHEMICAL, BVBA (EMPC) 
 POLDERDIJKWEG  
B-2030 Antwerpen
Belgium

24 Hour Environmental / Health Emergency Telephone | (UK) 01372 222 000 / (IRELAND) 44 1372 222 000
e-mail | SDS-UK@EXXONMOBIL.COM

SECTION 2 | HAZARDS IDENTIFICATION
 
This material is not considered to be hazardous according to regulatory guidelines see Section 15.

 

HEALTH HAZARDS
 Low order of toxicity.  Excessive exposure may result in eye, skin, or respiratory irritation.  High-pressure injection under skin may cause serious damage.

Note:   This material should not be used for any other purpose than the intended use in Section 1 without expert advice. Health studies have shown that chemical exposure may cause potential human health risks which may vary from person to person.  

SECTION 3 | COMPOSITION / INFORMATION ON INGREDIENTS
 
No Reportable Hazardous Substance(s) or Complex Substance(s).    

SECTION 4 | FIRST AID MEASURES

INHALATION
 Remove from further exposure.  For those providing assistance, avoid exposure to yourself or others.  Use adequate respiratory protection.  If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek immediate medical assistance.  If breathing has stopped, assist ventilation with a mechanical device or use mouth-to-mouth resuscitation.

SKIN CONTACT
 Wash contact areas with soap and water.  If product is injected into or under the skin, or into any part of the body, regardless of the appearance of the wound or its size, the individual should be evaluated immediately by a physician as a surgical emergency. Even though initial symptoms from high pressure injection may be minimal or absent, early surgical treatment within the first few hours may significantly reduce the ultimate extent of injury.

EYE CONTACT
 Flush thoroughly with water.  If irritation occurs, get medical assistance.

INGESTION
 First aid is normally not required. Seek medical attention if discomfort occurs.

 

SECTION 5 | FIRE FIGHTING MEASURES

EXTINGUISHING MEDIA
Appropriate Extinguishing Media:  Use water fog, foam, dry chemical or carbon dioxide (CO2) to extinguish flames.

Inappropriate Extinguishing Media:  Straight streams of water

FIRE FIGHTING
Fire Fighting Instructions:  Evacuate area.  Prevent run-off from fire control or dilution from entering streams, sewers or drinking water supply.  Fire-fighters should use standard protective equipment and in enclosed spaces, self-contained breathing apparatus (SCBA).   Use water spray to cool fire exposed surfaces and to protect personnel.  

Hazardous Combustion Products:   Smoke, Fume, Aldehydes, Sulphur Oxides, Incomplete combustion products, Oxides of carbon

FLAMMABILITY PROPERTIES 
Flash Point [Method]:  >205C  (401F) [ ASTM D-92]
Flammable Limits (Approximate volume % in air):   LEL:  0.9     UEL: 7.0
Autoignition Temperature:  N/D 

SECTION 6 | ACCIDENTAL RELEASE MEASURES

NOTIFICATION PROCEDURES
 In the event of a spill or accidental release, notify relevant authorities in accordance with all applicable regulations.

SPILL MANAGEMENT
Land Spill:  Stop leak if you can do so without risk.  Recover by pumping or with suitable absorbent.

Water Spill:  Stop leak if you can do so without risk.  Confine the spill immediately with booms.   Warn other shipping.   Remove from the surface by skimming or with suitable absorbents.   Seek the advice of a specialist before using dispersants.

Water spill and land spill recommendations are based on the most likely spill scenario for this material; however, geographic conditions, wind, temperature, (and in the case of a water spill) wave and current direction and speed may greatly influence the appropriate action to be taken.  For this reason, local experts should be consulted.  Note:  Local regulations may prescribe or limit action to be taken. 

ENVIRONMENTAL PRECAUTIONS
 Large Spills:  Dyke far ahead of liquid spill for later recovery and disposal.  Prevent entry into waterways, sewers, basements or confined areas.

SECTION 7 | HANDLING AND STORAGE

HANDLING
  Prevent small spills and leakage to avoid slip hazard.       

Static Accumulator:   This material is a static accumulator.

STORAGE
Do not store in open or unlabelled containers.  Keep away from incompatible materials.           

SECTION 8 | EXPOSURE CONTROLS / PERSONAL PROTECTION

  

Exposure limits/standards for materials that can be formed when handling this product:   When mists / aerosols can occur, the following are recommended:  5 mg/m³ - ACGIH TLV,  10 mg/m³ - ACGIH STEL.     
 
Note: Information about recommended monitoring procedures can be obtained from the relevant agency(ies)/institute(s): 
 UK               Health and Safety Executive (HSE)
ENGINEERING CONTROLS

The level of protection and types of controls necessary will vary depending upon potential exposure conditions. Control measures to consider:
 No special requirements under ordinary conditions of use and with adequate ventilation. 

PERSONAL PROTECTION
 
Personal protective equipment selections vary based on potential exposure conditions such as applications, handling practices, concentration and ventilation.  Information on the selection of protective equipment for use with this material, as provided below, is based upon intended, normal usage.  

Respiratory Protection:   If engineering controls do not maintain airborne contaminant concentrations at a level which is adequate to protect worker health, an approved respirator may be appropriate.  Respirator selection, use, and maintenance must be in accordance with regulatory requirements, if applicable.  Types of respirators to be considered for this material include: 
 No special requirements under ordinary conditions of use and with adequate ventilation.   

For high airborne concentrations, use an approved supplied-air respirator, operated in positive pressure mode.  Supplied air respirators with an escape bottle may be appropriate when oxygen levels are inadequate, gas/vapour warning properties are poor, or if air purifying filter capacity/rating may be exceeded.

Hand Protection:   Any specific glove information provided is based on published literature and glove manufacturer data.  Glove suitability and breakthrough time will differ depending on the specific use conditions. Contact the glove manufacturer for specific advice on glove selection and breakthrough times for your use conditions. Inspect and replace worn or damaged gloves. The types of gloves to be considered for this material include:
 No protection is ordinarily required under normal conditions of use.  

Eye Protection:   If contact is likely, safety glasses with side shields are recommended.

Skin and Body Protection:    Any specific clothing information provided is based on published literature or manufacturer data.  The types of clothing to be considered for this material include:
 No skin protection is ordinarily required under normal conditions of use.  In accordance with good industrial hygiene practices, precautions should be taken to avoid skin contact.

Specific Hygiene Measures:   Always observe good personal hygiene measures, such as washing after handling the material and before eating, drinking, and/or smoking.  Routinely wash work clothing and protective equipment to remove contaminants.  Discard contaminated clothing and footwear that cannot be cleaned. Practice good housekeeping.

ENVIRONMENTAL CONTROLS
 See Sections  6,  7, 12, 13.
 
SECTION 9 | PHYSICAL AND CHEMICAL PROPERTIES

Typical physical and chemical properties are given below.   Consult the Supplier in Section 1 for additional data.

GENERAL INFORMATION
Physical State:    Liquid 
Colour:   Amber
Odour:   Characteristic
Odour Threshold:   N/D

IMPORTANT HEALTH, SAFETY, AND ENVIRONMENTAL INFORMATION
Relative Density (at 15 C):    0.883   
Flash Point [Method]:     >205C  (401F) [ ASTM D-92]
Flammable Limits (Approximate volume % in air):   LEL:  0.9     UEL: 7.0  
Autoignition Temperature:  N/D 
Boiling Point / Range:    > 316C  (600F)
Vapour Density (Air = 1):   > 2 at 101 kPa
Vapour Pressure:   < 0.013 kPa (0.1 mm Hg) at 20°C
Evaporation Rate (N-Butyl Acetate = 1):   N/D
pH:   N/A
Log Pow (n-Octanol/Water Partition Coefficient):   > 3.5
Solubility in Water:   Negligible
Viscosity:   32 cSt  (32 mm²/sec) at 40°C  |  5.27 cSt  (5.27 mm²/sec) at 100C
Oxidising properties:  See Sections 3, 15, 16.

OTHER INFORMATION
Freezing Point:   N/D
Melting Point:   N/A
Pour Point:      -6°C  (21°F)   
DMSO Extract (mineral oil only), IP-346:    < 3 %wt 

SECTION 10 | STABILITY AND REACTIVITY

STABILITY:  Material is stable under normal conditions.

CONDITIONS TO AVOID:  Excessive heat. High energy sources of ignition.

MATERIALS TO AVOID:   Strong oxidisers

HAZARDOUS DECOMPOSITION PRODUCTS:  Material does not decompose at ambient temperatures.

HAZARDOUS POLYMERIZATION:  Will not occur.

SECTION 11 | TOXICOLOGICAL INFORMATION

Acute Toxicity

Route of Exposure | Conclusion / Remarks
INHALATION |
Toxicity: LC50 > 5000 mg/m3 | Minimally Toxic. Based on test data for structurally similar materials.
Irritation: No end point data. | Negligible hazard at ambient/normal handling temperatures. Based on assessment of the components.
INGESTION |
Toxicity: LD50 > 5000 mg/kg | Minimally Toxic. Based on test data for structurally similar materials.
Skin |
Toxicity: LD50 > 5000 mg/kg | Minimally Toxic. Based on test data for structurally similar materials.
Irritation: Data available. | Negligible irritation to skin at ambient temperatures. Based on test data for structurally similar materials.
Eye |
Irritation: Data available. | May cause mild, short-lasting discomfort to eyes. Based on test data for structurally similar materials.

CHRONIC/OTHER EFFECTS
 Contains:
Base oil severely refined:  Not carcinogenic in animal studies. Representative material passes IP-346, Modified Ames test, and/or other screening tests. Dermal and inhalation studies showed minimal effects; lung non-specific infiltration of immune cells, oil deposition and minimal granuloma formation. Not sensitising in test animals.

Additional information is available by request.

SECTION 12 | ECOLOGICAL INFORMATION

The information given is based on data available for the material, the components of the material, and similar materials.

ECOTOXICITY   
             Material -- Not expected to be harmful to aquatic organisms. 

MOBILITY 
             Base oil component -- Low solubility and floats and is expected to migrate from water to the land.  Expected to partition to sediment and wastewater solids. 

PERSISTENCE AND DEGRADABILITY
Biodegradation: 
             Base oil component --  Expected to be inherently biodegradable   

BIOACCUMULATION POTENTIAL 
             Base oil component -- Has the potential to bioaccumulate, however metabolism or physical properties may reduce the bioconcentration or limit bioavailability.

    

 
 
SECTION 13 | DISPOSAL CONSIDERATIONS
 
Disposal recommendations based on material as supplied.  Disposal must be in accordance with current applicable laws and regulations, and material characteristics at time of disposal. 

DISPOSAL RECOMMENDATIONS
 Product is suitable for burning in an enclosed controlled burner for fuel value or disposal by supervised incineration at very high temperatures to prevent formation of undesirable combustion products. 
 
REGULATORY DISPOSAL INFORMATION 

European Waste Code:  13 02 05

NOTE:  These codes are assigned based upon the most common uses for this material and may not reflect contaminants resulting from actual use.  Waste producers need to assess the actual process used when generating the waste and its contaminants in order to assign the proper waste disposal code(s).

This material is considered as hazardous waste pursuant to Directive 91/689/EEC on hazardous waste, and subject to the provisions of that Directive unless Article 1(5) of that Directive applies.

 Empty Container Warning Empty Container Warning (where applicable):  Empty containers may contain residue and can be dangerous.  Do not attempt to refill or clean containers without proper instructions.  Empty drums should be completely drained and safely stored until appropriately reconditioned or disposed.  Empty containers should be taken for recycling, recovery, or disposal through suitably qualified or licensed contractor and in accordance with governmental regulations.  DO NOT PRESSURISE, CUT, WELD, BRAZE, SOLDER, DRILL, GRIND, OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME, SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION.  THEY MAY EXPLODE AND CAUSE INJURY OR DEATH.

SECTION 14 | TRANSPORT INFORMATION

LAND (ADR/RID) :  Not Regulated for Land Transport
                  
INLAND WATERWAYS (ADNR) :  Not Regulated for Inland Waterways Transport

SEA (IMDG) :  Not Regulated for Sea Transport according to IMDG-Code

AIR (IATA) :  Not Regulated for Air Transport

SECTION 15 | REGULATORY INFORMATION

Material is not dangerous as defined by the EU Dangerous Substances/Preparations Directives.

EU LABELING:  Not regulated according to EC Directives
 
. | | |
. | | |

REGULATORY STATUS AND APPLICABLE LAWS AND REGULATIONS

Complies with the following national/regional chemical inventory requirements:   AICS, IECSC, DSL, EINECS, ENCS, KECI, PICCS, TSCA
  
SECTION 16 | OTHER INFORMATION

N/D = Not determined, N/A = Not applicable

THIS SAFETY DATA SHEET CONTAINS THE FOLLOWING REVISIONS:
Revision Changes:
Section 06: Notification Procedures - Header was modified.
Section 13: Empty Container Warning was modified.
Section 09: Phys/Chem Properties Note was modified.
Section 09: Boiling Point ºC(ºF) was modified.
Section 08: Hand Protection was modified.
Section 08: Environmental Control - Note was modified.
Section 07: Handling and Storage - Storage Phrases was modified.
Section 05: Hazardous Combustion Products was modified.
Section 06: Accidental Release - Spill Management - Water was modified.
Section 09: Relative Density - Header was modified.
Section 09: Flash Point ºC(ºF) was modified.
Section 09: Viscosity was modified.
Section 08: Environmental Control - Note was modified.
Section 16: Code to MHCs was modified.
Section 11: Oral Lethality Test Data was modified.
Section 11: Dermal Lethality Test Data was modified.
Section 01: Company Contact Methods Sorted by Priority was modified.

  
-----------------------------------------------------------------------------------------------------------------------------------------------------
The information and recommendations contained herein are, to the best of ExxonMobil's knowledge and belief, accurate and reliable as of the date issued.  You can contact ExxonMobil to insure that this document is the most current available from ExxonMobil.  The information and recommendations are offered for the user's consideration and examination.  It is the user's responsibility to satisfy itself that the product is suitable for the intended use.  If buyer repackages this product, it is the user's responsibility to insure proper health, safety and other necessary information is included with and/or on the container.  Appropriate warnings and safe-handling procedures should be provided to handlers and users.  Alteration of this document is strictly prohibited.  Except to the extent required by law, re-publication or retransmission of this document, in whole or in part, is not permitted.  The term, "ExxonMobil" is used for convenience, and may include any one or more of ExxonMobil Chemical Company, Exxon Mobil Corporation, or any affiliates in which they directly or indirectly hold any interest.

-----------------------------------------------------------------------------------------------------------------------------------------------------
Internal Use Only |
MHC:  0B, 0B, 0, 0, 0, 0 | PPEC:   A

 DGN:  2007218XGB  (547757)
-----------------------------------------------------------------------------------------------------------------------------------------------------